RIPE

NCC

August 1997 - IETF Aut-num Authorization in the RR 1

$ XW

�

Q XP

�$ XWK RUL] DWLRQ� IRU

5RX WH�2 EMHFWV

LQ� WKH�5 5

Carol Orange

RIPE NCC

RIPE

NCC

* RD O

Allow network operators to control

and monitor the registration of

route objects with their AS

specified in the ^origin:~ attribute.

Non-Goal :

Produce an optimal hierarchical

authorisation scheme for the RR

RIPE

NCC

August 1997 - IETF Aut-num Authorization in the RR 3

([ DP S OH aut - num : AS3333 mnt -route: AS333-MNT mntner : AS333-MNT auth : CRYPT-PW peEw8Gb4xBNqI route: 193.0.0.0/23

�