10 Repeat step 6 to 8

on this flap Repeat these steps on all other flaps

11 12

13 Open model using

existing creases

14 ’Crimp’

15 Block crimpfold 16

17 Open 18 Crimp