7. X-Ray view,reverse fold

thetwo flaps. Repeat on other

threesides.

8. Pleat sink the tw o flaps.

Repeat on the other three

sides.

9. Nolonger an X-Ray view.

Pull pointAallthe way down

asfaras itw ill go, thinningthe

diagonalsas youfold.

A

Br ai ded Pa pe r -

J. C. No la n 2/13 /92

4. Following the existing creases,

start to fold a windmillbase, bringing

points AandB to the center.

5. Tocomplete thebase,

do the samewith C& D.

A

B

C

D

1. Fold and unfold laterally. 2. Fold and unfold infourths.

Turnover.

3. Fold andunfold.Turn over.

B

A

6.This is a completed windmill

base. Sinkallfour corners.

Hi gh Int erme diat e dif ficul ty le vel. A 10 " pie ce of pap er produ ces a 3 3/4" mode l.

10. Repeat on the next flap.

PointAw ill becom e covered.

A

B

11. Repeat on the next flap. 12. Repeat on the last flap, tucking

the endinsidewhen done.

13. The first level is complete. 14. Fold thenext flap dow n. 15. ...and thenext flap...

16. ...andthenext flap... 17. ...and thefinal flap, folding

over the first flap, underthe next,

and out the otherside.

18. Completed model.

A

B

C

B

C

A

D

D

A

C

B

E

E

F

E

F

G

F

E

G

B

B