-- --

IEEE P1003.2 Draft 11.2 - September 1991

Copyright � 1991 by the Institute of Electrical and Electronics Engineers, Inc. 345 East 47th Street New York, NY 10017, USA All rights reserved as an unpublished work.

This is an unapproved and unpublished IEEE Standards Draft, subject to change. The publication, distribution, or copying of this draft, as well as all derivative works based on this draft, is expressly prohibited except as set forth below.

Permission is hereby granted for IEEE Standards Committee participants to reproduce this document for purposes of IEEE standardization activities only, and subject to the restrictions contained herein.

Permission is hereby also granted for member bodies and technical committees of ISO and IEC to reproduce this document for purposes of developing a national position, subject to the restrictions contained herein.

Permission is hereby also granted to the preceding entities to make limited copies of this document in an electronic form only for the stated activities.

The following restrictions apply to reproducing or transmitting the document in any form: 1) all copies or portions thereof must identify the document’s IEEE project number and draft number, and must be accompanied by this entire notice in a prominent location; 2) no portion of this document may be redistributed in any modified or abridged form without the prior approval of the IEEE Standards Department.

Other entities seeking permission to reproduce this document, or any portion thereof, for standardization or other activities, must contact the IEEE Standards Department for the appropriate license.

Use of information contained in this unapproved draft is at your own risk.

IEEE Standards Department Copyright and Permissions 445 Hoes Lane, P.O. Box 1331 Piscataway, NJ 08855-1331, USA +1 (908) 562-3800 +1 (908) 562-1571 [FAX]

-- --

P1003.2/D11.2 INFORMATION TECHNOLOGY—POSIX

8037 4.37 logname — Return user’s login name

8038 4.37.1 Synopsis

8039 logname

8040 4.37.2 Description

8041 The logname utility shall write the user’s login name to standard output. The 8042 login name shall be the string that would be returned by the POSIX .1 {8}getlo- 8043 gin () function. Under the conditions where the getlogin () function would fail, the 8044 logname utility shall write a diagnostic message to standard error and exit with 8045 a nonzero exit status.

8046 4.37.3 Options

8047 None.

8048 4.37.4 Operands

8049 None.

8050 4.37.5 External Influences

8051 4.37.5.1 Standard Input

8052 None.

8053 4.37.5.2 Input Files

8054 None.

8055 4.37.5.3 Environment Variables

8056 The following environment variables shall affect the execution of logname :

8057 LANG This variable shall determine the locale to use for the 8058 locale categories when both LC_ALL and the correspond- 8059 ing environment variable (beginning with LC_) do not 8060 specify a locale. See 2.6.

8061 LC_ALL This variable shall determine the locale to be used to over- 8062 ride any values for locale categories specified by the set- 8063 tings of LANG or any environment variables beginning 8064 with LC_.

Copyright � 1991 IEEE. All rights reserved. This is an unapproved IEEE Standards Draft, subject to change.

494 4 Execution Environment Utilities

Part 2: SHELL AND UTILITIES P1003.2/D11.2 8065 LC_MESSAGES This variable shall determine the language in which mes- 8066 sages should be written. 8067 4.37.5.4 Asynchronous Events 8068 Default.

8069 4.37.6 External Effects 8070 4.37.6.1 Standard Output 8071 The logname utility output shall be a single line consisting of the user’s login 8072 name: 8073 "%s\n" , <login name> 8074 4.37.6.2 Standard Error 8075 Used only for diagnostic messages. 8076 4.37.6.3 Output Files 8077 None.

8078 4.37.7 Extended Description 8079 None.

8080 4.37.8 Exit Status 8081 The logname utility shall exit with one of the following values: 8082 0 Successful completion. 8083 >0 An error occurred.

8084 4.37.9 Consequences of Errors 8085 Default.

Copyright � 1991 IEEE. All rights reserved. This is an unapproved IEEE Standards Draft, subject to change.

4.37 logname — Return user’s login name 495

P1003.2/D11.2 INFORMATION TECHNOLOGY—POSIX

8086 4.37.10 Rationale. (This subclause is not a part of P1003.2)

8087 Examples, Usage

8088 The logname utility explicitly ignores the LOGNAME environment variable 8089 because environment changes could produce erroneous results.

8090 History of Decisions Made

8091 The passwd file is not listed as required, because the implementation may have 8092 other means of mapping login names.

8093 4.38 lp — Send files to a printer

8094 4.38.1 Synopsis

8095 lp [- c ] [- d dest ] [- n copies ] [file ... ]

8096 4.38.2 Description

8097 The lp utility shall copy the input files to an output device in an unspecified 8098 manner. The default output destination should be to a hardcopy device, such as a 8099 printer or microfilm recorder, that produces nonvolatile, human-readable docu- 8100 ments. If such a device is not available to the application, or if the system pro- 8101 vides no such device, the lp utility shall exit with a nonzero exit status.

8102 The actual writing to the output device may occur some time after the lp utility 8103 successfully exits. During the portion of the writing that corresponds to each 8104 input file, the implementation shall guarantee exclusive access to the device.

8105 4.38.3 Options

8106 The lp utility shall conform to the utility argument syntax guidelines described 8107 in 2.10.2.

8108 The following options shall be supported by the implementation:

8109 - c Exit only after further access to any of the input files is no longer 8110 required. The application can then safely delete or modify the 8111 files without affecting the output operation.

8112 - d dest Specify a string that names the output device or destination. If 8113 - d is not specified, and neither the LPDEST nor PRINTER 8114 environment variable is set, an unspecified output device is used. 8115 The - d dest option shall take precedence over LPDEST , which in 8116 turn shall take precedence over PRINTER . Results are undefined 8117 when dest contains a value that is not a valid device or

Copyright � 1991 IEEE. All rights reserved. This is an unapproved IEEE Standards Draft, subject to change.

496 4 Execution Environment Utilities