IEEE P1003.2a Draft 8 - December 1991

Copyright � 1991 by the Institute of Electrical and Electronics Engineers, Inc. 345 East 47th Street New York, NY 10017, USA All rights reserved as an unpublished work.

This is an unapproved and unpublished IEEE Standards Draft, subject to change. The publication, distribution, or copying of this draft, as well as all derivative works based on this draft, is expressly prohibited except as set forth below.

Permission is hereby granted for IEEE Standards Committee participants to reproduce this document for purposes of IEEE standardization activities only, and subject to the restrictions contained herein.

Permission is hereby also granted for member bodies and technical committees of ISO and IEC to reproduce this document for purposes of developing a national position, subject to the restrictions contained herein.

Permission is hereby also granted to the preceding entities to make limited copies of this document in an electronic form only for the stated activities.

The following restrictions apply to reproducing or transmitting the document in any form: 1) all copies or portions thereof must identify the document’s IEEE project number and draft number, and must be accompanied by this entire notice in a prominent location; 2) no portion of this document may be redistributed in any modified or abridged form without the prior approval of the IEEE Standards Department.

Other entities seeking permission to reproduce this document, or any portion thereof, for standardization or other activities, must contact the IEEE Standards Department for the appropriate license.

Use of information contained in this unapproved draft is at your own risk.

IEEE Standards Department Copyright and Permissions 445 Hoes Lane, P.O. Box 1331 Piscataway, NJ 08855-1331, USA +1 (908) 562-3800 +1 (908) 562-1571 [FAX]

PART 2: SHELL AND UTILITIES — Amd. 1: UPE P1003.2a/D8

1101 variable in System V mailx , although it has not been documented in the SVID . 7

1102 The indentprefix variable, the retain and unalias commands, and the ~F 7 1103 and ~Mcommand escapes were adopted from 4.3BSD Mail . 7

1104 The version command was not included because no sufficiently general 1105 specification of the version information could be devised that would still be useful 1106 to a portable user. This command name should be used by suppliers who wish to 1107 provide version information about the mailx command.

1108 The ‘‘implementation-specific (unspecified) system startup file’’ has been tradition- 7 1109 ally named /etc/mailx.rc , but this specific name and location are not required.

1110 4.52 read — Read a line from standard input

1111 � 4.52.2 read Description. In subclause 4.52, add the following to the end of 1112 the second paragraph in the Description subclause:

1113 If standard input is a terminal device and the invoking shell is interactive, 1114 read shall prompt for a continuation line when:

1115 — The shell reads an input line ending with a backslash, unless the - r option 1116 is specified.

1117 — A here-document is not terminated after a <newline> is entered.

1118 � 4.52.5.3 read Environment Variables. In subclause 4.52, add the follow- 1119 ing environment variable in the correct sorted order to the Environment Vari- 1120 ables subclause.

1121 PS 2 This variable shall contain the prompt string that an interac- 1122 tive shell shall write to standard error when a line ending 1123 with a backslash is read and the - r option was not specified, 1124 or if a here-document is not terminated after a <newline> is 1125 entered.

1126 � 4.51.6.2 read Standard Error. In subclause 4.52, replace the Standard 1127 Error subclause with the following.

1128 Used for diagnostic messages and prompts for continued input.

Copyright � 1991 IEEE. All rights reserved. This is an unapproved IEEE Standards Draft, subject to change.

4.52 read — Read a line from standard input 57

P1003.2a/D8 INFORMATION TECHNOLOGY—POSIX

1129 Rationale. (This subclause is not a part of P1003.2a)

1130 None.

1131 4.56 sh — Shell, the standard command language interpreter

1132 � 4.56.1 sh Synopsis. Add the - b, - m, and - o option options to each of the 1133 three Synopsis lines with appropriate editorial wording indicating that these 7 1134 options need to be supported only when the UPUO is supported: 7

1135 � 4.56.3 sh Options. Change the first sentence of the second paragraph, begin- 1136 ning ‘‘The - a, - C, ... ’’to:

1137 The - a, - b, - C, - e, - f , - m, - n, - o option , - u, - v, and - x options are described 1138 as part of the set utility in 3.14.11.

1139 � 4.56.3 sh Options. Remove the following sentence and NOTE: 8

1140 The behavior of an interactive shell is not fully specified by this standard. 8 1141 NOTE: The preceding sentence is expected to change following the eventual approval of the UPE 8 1142 supplement. 8

1143 � 4.56.5.3 sh Environment Variables. Modify the contents of subclause 1144 4.56.5.3, Environment Variables, to add the following environment variables in 1145 the correct sorted order.

1146 FCEDIT 8 1147 HISTFILE 8 1148 HISTSIZE See the description of the fc environment variables in 8 1149 5.12.5.3. This standard specifies the effects of these 8 1150 variables only for systems supporting the User Porta- 8 1151 bility Utilities Option. 8

1152 MAIL This variable shall be interpreted as a pathname of the 1153 user’s mailbox file for purposes of incoming mail 1154 notification. If this variable is set, the shell shall 1155 inform the user if the file named by the variable is 1156 created or if its modification time has changed. 1157 Informing the user shall be accomplished by writing a 1158 string of unspecified format to the standard error prior 1159 to the writing of the next primary prompt string after 1160 the completion of an interval defined by the MAIL- 1161 CHECK variable. The user shall be informed only if 1162 MAIL is set and MAILPATH is not set. This standard 7

Copyright � 1991 IEEE. All rights reserved. This is an unapproved IEEE Standards Draft, subject to change.

58 4 Revisions to Execution Environment Utilities